{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":20,"n_cols":8,"rows_kept":20,"merged":[[0,0,0,7],[1,0,1,7],[2,0,2,7],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,3,6],[3,7,4,7],[6,1,8,1],[11,1,12,1],[13,1,14,1],[17,1,18,1],[19,0,19,7]]}
["报价表"]
["报价单位（加盖公章）：                                                          年    月     日"]
["联系人：                                         联系电话："]
["序号","物资/服务名称","规格或型号","单位","数量","金额（元，含税及运费）",null,"备注"]
[{"$nulls":5},"单价      ","总价     "]
[1,"门口主题公园立牌","钢结构镀锌板烤漆造型 单面宽100cm*高220cm 混凝土预埋安装 ","座",1]
[2,"版面更换\n（公园入口右侧）","300x120cm 户外高清防水贴","张",1]
[3,null,"125x95cm 户外高清车贴+板","张",1]
[4,null,"275x110cm 户外高清车贴 ","张",1]
[5,"版面更换\n（停车场保安亭处）","238X118cm 户外高清车贴+板","张",1]
[6,"防震互动牌","钢结构镀锌板烤漆造型 单面宽260cm*高250cm 混凝土预埋安装 ","座",1]
[7,"版面更换\n（中国地震监测处）","225x120cm 户外高清车贴+板","张",1]
[8,null,"161X92cm 户外高清车贴+板","张",4]
[9,"地震仪模型","底座直径1.6米，高1.2米\n青铜手工定做，（玻璃钢）高分子复合材料，采用多层网状玻璃纤维布，手糊成形，不易龟裂变形。采用户外汽车漆喷涂。","座",1]
[10,null,"底座直径200cm，高60cm，\n钢结构镀锌板喷漆造型 预埋安装 ","座",1]
[11,"电线杆灯箱","单面画面 宽50cm*高90cm  \n箱体镀锌板折弯 表面高温静电喷塑 视窗透明耐力板 LED侧光源 画面灯片","套",6]
[12,"版面更换\n（麒麟广场）","225x120cm 户外高清车贴+板","张",1]
[13,"地震监测局门口宣传栏版面更换","95X107cm  户外高清车贴+板","张",7]
[14,null,"285X107cm  户外高清车贴+板","张",1]
["合计：               元（含税及运费）"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}